// Copyright (C) 2025 The Qt Company Ltd.
// SPDX-License-Identifier: LicenseRef-Qt-Commercial OR GFDL-1.3-no-invariants-only

/*!
    \page creator-vxworks.html
    \previouspage creator-how-tos.html

    \title Developing for VxWorks

    \quotation
    \l {how-to-vxworks}{How to: Develop for VxWorks}
    \endquotation

    \summary {Use Qt for VxWorks to develop Qt applications for VxWorks
    embedded systems.}

    \note Enable the VxWorks plugin to use it.

    Run and debug applications on \l{VxWorks} devices. Currently, you can develop
    applications with Qt 6.8 and build them for VxWorks 24.03 devices.

    Create a connection between \QC and a VxWorks device. Then add the device to
    a VxWorks kit.

    For more information about how to configure the device and Qt, as well as how
    to develop applications, see \l {Qt for VxWorks}.

    \sa {Enable and disable plugins}, {how-to-vxworks}{How to: VxWorks},
    {Qt for VxWorks}
*/

/*!
    \page creator-how-to-create-vxworks-kits.html
    \previouspage creator-how-tos.html

    \ingroup creator-how-to-vxworks

    \title Create kits for VxWorks devices

    To develop Qt applications for VxWorks, build \l {Qt for VxWorks} and create
    a VxWorks \l {Managing kits}{kit}.

    \note Enable the VxWorks plugin to use it.

    To create a kit:

    \list 1
        \li Go to \preferences > \uicontrol Devices > \uicontrol VxWorks.
            \image {qtcreator-preferences-devices-vxworks.webp} {VxWorks tab in Devices preferences}
        \li In \uicontrol {VxWorks installation folder}, enter the path to the
            directory where WindRiver installer installed VxWorks.
        \li In \uicontrol {NFS export directory for VxWorks devices}, enter the
            path to an NFS directory shared with the device.
        \li Select \uicontrol {Add Kit}.
        \li In \uicontrol {Kit name}, enter a name for the kit.
            \image {qtcreator-create-new-kit-vxworks.webp} {Create New Kit dialog}
        \li In \uicontrol {Path}, select the folder that contains qmake for
            the Qt VxWorks build.
        \li In \uicontrol {VSB path}, enter the path to the VxWorks source build
            (VSB) directory.
        \li In \uicontrol {Hostname}, enter the host name or IP address of the
            device.
        \li In \uicontrol {Username}, enter the user name to access the device.
        \li Select \uicontrol OK to create a VxWorks kit.
        \li Go to \uicontrol Projects > \uicontrol {Build & Run} to activate the
            kit for your project.
    \endlist

    \note To deploy the built package, you can add a build step to the deploy
    configuration of the project that copies the built binary of your project to
    a NFS directory shared with the device.

    \sa {Enable and disable plugins}, {how-to-vxworks}{How to: VxWorks},
    {Developing for VxWorks}, {Qt for VxWorks}
*/

/*!
    \page creator-how-to-debug-vxworks.html
    \previouspage creator-how-tos.html

    \ingroup creator-how-to-vxworks
    \ingroup creator-how-to-debug

    \title Debug C++ applications on VxWorks devices

    \note Place all the library dependencies on the SD card. Debugging doesn't
    work from other locations, such as a mounted NFS directory.

    \QC only copies the application binaries and other deployable files to
    the root of the SD card. It doesn't preserve nor create the directory
    structure on the SD card.

    To debug Qt applications, add the following line to your VxWorks source build
    (VSB) configuration:

    \code [shell]
    vxprj vsb config -s -add "_WRS_CONFIG_TCF_GDB_RSP=y"
    \endcode

    To automatically start the GDB server on the device, add the following lines
    to your VxWorks image project (VIP) configuration:

    \code [text]
    "INCLUDE_DEBUG_AGENT"
    "INCLUDE_DEBUG_AGENT_START"
    "INCLUDE_STANDALONE_SYM_TBL"
    \endcode

    For more information, see \l {Qt for VxWorks}.

    To set up debugging:

    \list 1
        \li Activate a VxWorks kit for the project.
        \li Go to \uicontrol Projects > \uicontrol {Run Settings}.
        \li Set \uicontrol Priority and \uicontrol {Stack size}.
            \image {qtcreator-run-settings-vxworks.webp} {Run Settings for VxWorks}
        \li In \uicontrol Environment, set the \c LD_LIBRARY_PATH variable to
            the location of the libraries on the SD card. If the path to the
            SD card is not \c {/sd0a}, set \c VX_SDCARD_PATH to the correct
            location.
    \endlist

    To start debugging, select \key {F5} or go to \uicontrol Debug >
    \uicontrol {Start Debugging} > \uicontrol {Start Debugging of Startup Project}.

    \sa {Activate kits for a project}, {Enable and disable plugins},
    {how-to-vxworks}{How to: VxWorks}, {Debugging}, {Developing for VxWorks},
    {Qt for VxWorks}
*/

/*!
    \page creator-how-to-connect-vxworks-ssh.html
    \previouspage creator-how-tos.html

    \ingroup creator-how-to-vxworks

    \title Create SSH connections to VxWorks devices

    To run an SSH server on the VxWorks device, you need to configure it, as
    described in the following sections.

    \note Enable the VxWorks plugin to use it.

    \section1 Configure the VxWorks source build

    Set the following keys in the VxWorks Source Build (VSB):

    \code [text]
    "USER_MANAGEMENT"
    "USER_MANAGEMENT_USER_PRIVILEGES"
    \endcode

    \section1 Configure the VxWorks kernel

    Add the following includes to the VxWorks Kernel configuration (VIP):

    \code [text]
    "INCLUDE_IPSSH_CLIENT_CMD"
    "INCLUDE_SHELL_SECURITY"
    "INCLUDE_USER_DATABASE"
    "INCLUDE_USER_IDENTIFICATION"
    "INCLUDE_USER_PRIVILEGES"
    "INCLUDE_USER_MGT_SHELL_CMD"
    "INCLUDE_SEC_KEY_STORE_CMD"
    "INCLUDE_SHELL"
    "INCLUDE_SSH"
    "INCLUDE_IPD_CMD"
    \endcode

    \section1 Create a startup script

    In the startup script, set up user management and starting the SSH server.

    An example startup script:

    \code [text]
    cp "/romfs/ssh/keys/WindRiver.pk2","/ram"
    cmd keyStore import default_rsa /romfs/ssh/keys/default_rsa.pem
    cmd keyStore import default_dsa /romfs/ssh/keys/default_dsa.pem
    cmd ipd start ipssh
    udbReset
    userAdd "WindRiver","vxTarget"
    \endcode

    \section1 Test the connection

    To test the connection from the terminal, specify the key algorithms for it
    (because VxWorks uses old keys):

    \code [shell]
    ssh -oHostKeyAlgorithms=+ssh-rsa -lWindRiver 192.168.0.3
    \endcode

    \sa {Enable and disable plugins}, {how-to-vxworks}{How to: VxWorks},
    {Debugging}, {Developing for VxWorks}, {Qt for VxWorks}
*/
